Here you find SolidWorks Part file .SLDPRT of the 4-leg Birdcage coil holder.
The coil holder is split in smaller pieces for convenient 3D printing in conventional small-size printers.

Created by Jóan Hofgaard Køtlum.

If you use this design, credit must be given by referencing the following paper:

Jóan Hofgaard Køtlum, Mark Gosselink, Hans Hoogduin, Dennis Klomp, Vitaliy Zhurbenko, "Magnetically Coupled, Passive Birdcage Resonator for Boosting Sensitivity of 1.5T MRI," Proceedings of the European Microwave Week 2024, Paris.